HOW TO INSTALL GDOS64 ON YOUR ULTIMATE DEVICE

Check text to see if wording can be simplified for less technical folks

What you need

The GEOS 2.0 Boot Disk

The GDOS64 installation disk and name it GDOS64 Boot

A second copy of the GDOS64 installation disk to use later

Enable Drive A and set it as a 1541 drive

Enable Drive B and set it as a 1581 drive

Enable REU and set to at least 512MB (larger is better!)

Installing GDOS64

Start GEOS on drive A

Mount the GDOS64 installer (which you named GDOS64 Boot) on drive B

Copy the file Desk Top from drive A to drive B. The installer will check if this file is present!

Start the GDOS64 installer and install to B.

Install all system files, and only install the drivers for the 1541 and 1581 drives. More can be added after the installation completes.

Choose “Continue with installation”

Choose “Check system files”

You will be warned that some non-essential files are missing. Ignore and continue with installation.

You will be asked to install a new mouse driver. Answering “YES” will install and activate the new driver.

Installation will now complete, and after configuring the drives, GDOS64 will boot into its desktop.

You can now remove the installer files from the GDOS boot disk to make space.

And finally...

To add new drivers and other additional files, like a graphical background and accessories, boot GDOS64 from its boot disk, mount the second copy of the install disk, and restart the installation. You will be asked if you want to update. Answer YES, and you can install all the additional files.